**441/2--2019**

**HOMESCIENCE.**

**CLOTHING CONSTRUCTION.**

**PAPER 2**

**PRACTICAL**

**MARKING SCHEME.**

**CANDIDATE’S NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ INDEX NO. \_\_\_\_\_\_\_\_\_\_\_\_\_**

**TEACHER’S NAME:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **PROCESS** | **MAX SCORE (Marks)** | **CANDIDATE’S SCORE** | **REMARKS** |
| 1  a  b  c | **PRESENTATION**  Work well pressed (½) and well folded (½)  Label (½) firmly stitched (1) without concealing details (½) and on single fabric (½)  Pins/needles (½) and unnecessary threads (½), loose threads (½) removed. | 1  2½  1½ |  |  |
|  | **TOTAL** | **5** |  |  |
| a  b  c  d  e  f | **CUTTING OUT AND GRAIN**  Cut off all the 7 pieces.  Smooth cutting (1) of dress front and on straight grain on C. F (1) to within 2mm)  Smooth cutting (1) of dress back and on straight grain on CB (1)  Smooth cutting (1) of the collar (½) under collar (½) and interfacing (½) and on straight grain (1½).  Smooth cutting of back facing (½) and on grain (½)  Smooth cutting of binding (½) | 3½  2  2  3  1  ½ |  |  |
|  | **TOTAL** | **12** |  |  |
| a  b  c  d  e  f | **DOUBLE POINTED / FULL DART**  Straight stitching (½) X2) tapering to nothing (½) X 2) at both ends (½) X 2).  Approximately fastened at the points (1X 2)  Correct length (1) to within(+, - 2mm) (16cm)  Correct width of dart (widest part of (1cm) to 2mm (1).  Snipped (½) at the centre (½) and raw edge neatened (½) using appropriate stitches (½)  Flatness on R.S. (½) and on W. S. (½) | 3  2  1  1  2  1 |  |  |
|  | **TOTAL** | **10** |  |  |
| a  b  c  d  e | **DOUBLE STITCHED SHOULDER SEAM**  Straight stitching (1) of the first stitching line.  Each seam allowance trimmed to 6mm (1) and front to 12mm (1) even tucking under (1) and fell of the seam toward back of garment (1)  Evenness of the seam (1) and correct width (1) of the fell (0.6 – width +, - 2mm)  Straight stitchery of 2nd line of stitching (1) and close to the edge (1).  Flatness of the seam R.S. (½) and on WS (½) | 1  4  2  2  **1** |  |  |
|  | **TOTAL** | **10** |  |  |
| a  b  c  d | **SIDE SEAM (OPEN SEAM)**  (If not open seam award zero (0)  Seam joined with straight stitchery (2)  Well neatened raw edge (2x2)  Evenness of seam allowance (3)  Correct size of seam allowance (1cm) to within 2mm (0.8 – 1.2 cm) each side (2x2) | 2  4  3  4 |  |  |
|  | **TOTAL** | **13** |  |  |
| a  b  c  d | **FRONT AND BACK NECK FACINGS**  Extended front and back facings joined with straight stitchery (½) seam trimmed (½) pressed open (½) and unneatened (½)  Front facing folded back (½) on fold line (½) on garment held (1) with diagonal tacking (2) (left in place)  Joined facings neatened (1x2)  Catch stitched at the shoulder seam (1) | 2  4  2  1 |  |  |
|  | **TOTAL** | **9** |  |  |
| a  b  c  d  e  f  g  h  i  j | **COLLAR**  Smooth stitchery of outer edge of collar (1)  Collar seam trimmed (1) and snipped (1)  Well knife edged (2)  Collar attached by sandwiching (2) between garment and facing.  Quality of attaching stitchery on RS (1)  Attaching seam trimmed (1) and snipped (1)  Evenness of the collar (2)  Correct positioning of collar CF (1) flash with CF and CB with CB of collar (1)  Correct size (2) to within 3mm and  Correct shape (2) (superimpose pattern) | 1  2  2  2  1  2  2  2  2  **2** |  |  |
|  | **TOTAL** | **18** |  |  |
| a  b  c  d  e  f | **BINDING OF ARM HOLE**  Band correctly joined (1) with straight stitchery (1)  Raw edges of band well tucked under (1) and trimmed (1)  Band hemmed (1) for 6cm.  Quality of hemming stitch (density 1, depth 1)  Even width of band on RS (1) and WS (1)  (Correct depth of finished band (1.5cm + or -2mm LS (1) WS (1)).  Flatness of the band RS (½) and WS (½) | 2  2  1  2  2  2  **1** |  |  |
|  | **TOTAL** | **12** |  |  |
| a  b | **EDGE STITCHING OF THE HEM**  Edge neatened with straight stitchery (1)  Evenness of neatened edge (0.5cm ) (1) | 1  1 |  |  |
|  | **TOTAL** | **2** |  |  |
|  | **TOTAL 90 ÷ 2 = 45** |  |  |  |