**3.19** **POWER MECHANICS (447)**

**3.19.1  Power Mechanics Paper 1 (447/1)**

**SECTION A:**  (40 marks)

*Answer****all****the questions in this section*

**1** (a) List**three** factors to be considered when putting up a motor vehicle spare parts shop.

(3 marks)

(b) Explain**two** reasons why it is important to study power mechanics. (2 marks)

**2** (a) State the full terms represented by the following engineering drawing abbreviations:

(i) CL; ..........................................................................................................................

(ii) Ø; ............................................................................................................................

(iii) CSK; .......................................................................................................................

(iv) A/F. .........................................................................................................................

(2 marks)

(b) Name**two** classes of fire and for each class, identify**one** appropriate commercial fire

extinguisher. (2 marks)

**3** (a) State**two** advantages of self-tapping screws over ordinary screws. (2 marks)

(b) (i) Sketch an adjustable spanner. (1 mark)

(ii) State where long nose pliers may be used in a small engine. (1 mark)

**4** (a) Explain**one** purpose of each of the following energy convertors in a motor vehicle:

(i) alternator; (1 mark)

(ii) photo voltaic cells. (1 mark)

(b) State**two** effects of adding each of the following alloying materials to carbon steel:

(i) Nickel; (1 mark)

(ii) Molybdenum. (1 mark)

**5** With the aid of sketches,  differentiate between a 4 cylinder in line and a V-4 cylinder engine

block. (4 marks)

170

**6** Figure 1 shows a sectional view of a Wankel engine.  Describe**one** cycle of its operation with

reference to**C** and**D**. (4 marks)

**7** (a) Name the main components of the power transmission system of a motor vehicle.

(2 marks)

(b) Explain the reason why modern vehicles are designed with collapsible steering

columns. (2 marks)

**8** (a) Briefly explain the process of hard soldering. (3 marks)

(b) Explain the following terms as used in drum brake operation:

(i) leading shoe;

(ii) trailing shoe. (2 marks)

**9** (a) State the purpose of the ply-rating of a tyre. (2 marks)

(b) State**two** advantages of an independent suspension system over rigid beam suspension

system. (1 mark)

**10** Sketch a dipped beam light path having an offset filament and label its parts. (3 marks)

171

**SECTION B:** (60 marks)

*Answer question****11****and any other****three****questions.*

**11** Figure 2 shows an isometric view of a Vee block resting on one side.

Draw full size, in first angle projection, the following views:

(a) front elevation in the direction of arrow**W**;

(b) end elevation in the direction of arrow**X**;

(c) Plan.

(Use A3 paper provided) (15 marks)

172

(a) Name the component. ( 1  mark)

(b) Name parts labelled**A** to**G**. (3 1  marks)

**12** Figure 3 shows a component of the power transmission system of a motor vehicle.

2

2

(c) Explain how the component operates. (11 marks)

**13** With the aid of a labelled diagram, explain the operation of an overhead valve engine train

whose camshaft is in the engine block. (15 marks)

**14** With the aid of labelled diagrams, explain the operation of a four-stroke compression ignition

system. (15 marks)

**15** (a) State**three** advantages of disc brakes over drum brakes. (3 marks)

(b) Sketch a sectional diagram of a disc brake assembly and label six parts. (12 marks

173

**3.19.2  Power Mechanics Paper 2 (447/2)**

**1** STATION 1

In the space below, sketch in good proportion a sectional view of a mechanical fuel pump.

Label four major parts. (10 marks)

**2** STATION 2

Using the tools, equipment and materials provided, make the scoop shown in**figure 2**.

**Figure 2**

174

|  |  |  |  |
| --- | --- | --- | --- |
| **TOOL** | **NAME** | **ACCURACY** | **USAGE** |
| K |  |  |  |
| L |  |  |  |
| M |  |  |  |
| N |  |  |  |
| P |  |  |  |

**3** STATION 3

On the multi-coil clutch disc provided, perform the following operations:

(a) measure and record the:

(i) depth of the four marked rivets; (4 marks)

(ii) depth of the splines. (2 marks)

(b) Inspect the torsion spring for free play, or damage and comment. (2 marks)

(c) Inspect the friction surface for its service condition and comment. (2 marks)

**(Let the examiner check your work)**

**4** STATION 4

Identify the measuring tools labelled K to P and for each tool write the accuracy and two areas

where it is used.

**5** STATION 5

Using the tools and materials provided, connect a twin headlight parallel circuit controlled by a

single switch. (10 marks)

**Let the examiner check your work**.

175

|  |  |  |
| --- | --- | --- |
| **ITEM** | **NAME** | **USE** |
| A |  |  |
| B |  |  |
| C |  |  |
| D |  |  |
| E |  |  |
| F |  |  |
| G |  |  |
| H |  |  |
| I |  |  |
| J |  |  |

**6** STATION 6

Identify the tools and fasteners labelled A to J and state one use of each. (10 marks)

**7** STATION 7

On the single cylinder provided;

(a) Demonstrate to the examiner how to check the roundness of the camshaft using a dial

gauge.

(b) Count the number of teeth on the crankshaft and the camshaft and calculate the gear

ratio.

Crankshaft............................

teeth

teeth

Camshaft ............................

Gear ratio ............................ teeth

**8** STATION 8

(10 marks)

Carry out a compression test on the single cylinder engine provided and record the reading in

the space provided.

**(Let the examiner check your work).** (8 marks)

Compare your reading with the recommended reading provided by the examiner.

Comment on the state of the engine compression. (2 marks)

Comment:

176

**9** STATION 9

Identify the parts labelled P to T. For each part, identify ONE defect and ONE possible effect

on vehicle performance. Complete the table below.

**10** STATION 10

(10 marks)

Using the tools and materials provided perform the following operations on the mechanical fuel

pump provided.

(a) Dismantle the fuel pump. (2 marks)

(b) Check the service condition of each of the following parts and comment on each.

(i) Inlet valve; (2 marks)

(ii) diaphragm. (2 marks)

(c) Assemble the pump and test it using the fuel provided. (4 marks)

**(Let the examiner check your work)**

|  |  |  |  |
| --- | --- | --- | --- |
| **PART** | **NAME** | **DEFECT** | **EFFECT** |
| P |  |  |  |
| Q |  |  |  |
| R |  |  |  |
| S |  |  |  |
| T |  |  |  |