**441/2**

**HOME SCIENCE**

**(CLOTHING CONSTRUCTION)**

**PAPER 2**

**JANUARY 2021**

**K A S S U J O I N T E X A M I N A T I O N**

**JANUARY 2021**

**441/2**

**HOME SCIENCE**

**CLOTHING AND CONSTRUCTION**

**PAPER 2**

**MARKING SCHEME**

**Candidates Name: …………………………………………………………………………..**

**Index No.: ………………………………………**

**Subject Teacher’s Name: …………………………………………………………………**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | **TASKS** | **MAX. SCORE**  | **ACTUAL SCORE** | **REMARKS** |
| **1.** |  | **PRESENTATION** |  |  |  |
|  | (a) | Work well pressed and well folded | 1 |  |  |
|  | (b) | Label stitched on a single fabric  | 1  |  |  |
|  | (c) | Clearly written Name, Adm. No., Class | 1 ½  |  |  |
|  | (d) | Pins, unnecessaary tacking and hanging threads removed |  1 ½ |  |  |
|  | (e) | Made up left half  | 1 |  |  |
|  |  | **SUB TOTAL** | **6**  |  |  |
| **2.** |  | **CUTTING OUT** |  |  |  |
|  | (a) | All the ten pieces cut out. | 5 |  |  |
|  | (b) | Smooth cutting of the skirt back on straight grain at the CB. | 2 |  |  |
|  | (c) | Smooth cutting of the back bodice and on straight grain at CB. | 2 |  |  |
|  | (d) | Smooth cutting of the collar and on straight grain at the CB. | 4 |  |  |
|  | (e) | Smooth cutting of the back neck facing and on straight grain at the CB. | 2 |  |  |
|  |  | **SUB TOTAL** | **16** |  |  |
| **3.** |  | **SHOULDER SEAM *(Double stitched if not give zero)*** |  |  |  |
|  | (a) | Straight and firm stitchery of the first line. | 1 |  |  |
|  | (b) | Straight and firm stitchery of the second line close to the fold. |  1½  |  |  |
|  | (c) | Seam neatly tucked in to conceal the raw edges. |  ½  |  |  |
|  | (d) | Correct width (6 mm to within 2mm) | 1 |  |  |
|  | (e) | Fell folded to the back. | 1 |  |  |
|  | (f) | Seam flat on the W.S. & R.S | 1 |  |  |
|  | (g) | Evenness of complete seam. | ½  |  |  |
|  |  | **SUB TOTAL** | **6 ½** |  |  |
| **4.** |  | **SIDE SEAM *(Open seam, if not give zero)*** |  |  |  |
|  | (a) | Seam done with firm and straight stitchery. | 1 |  |  |
|  | (b) | Seam turnings neatened separately and appropriately. |  1 ½ |  |  |
|  | (c) | Correct size of the neatened turnings (1cm to within 2mm) |  1 |  |  |
|  | (d). | Evenness of the neatened turnings. | 1 |  |  |
|  | (e) | Seam pressed open and flat at the neckline. |  |  |  |
|  |  | **SUB TOTAL** | **4 ½** |  |  |
| **5.** |  | **JOINING THE FRONT AND BACK SKIRT TO THE JOINED BODICES *(Overlaid seam, if not give zero)*** |  |  |  |
|  | (a) | Gathers evenly distributed. | 1 |  |  |
|  | (b) | Forming gathers and not pleats. | 1/2 |  |  |
|  | (c) | Overlay bodice folded to the W.S at the stitching line.  | 1 |  |  |
|  | (d) | Overlay placed on the underlay (skirt) stitching line on the R.S | 1 |  |  |
|  | (e) | Seam stitched with straight and firm stitchery and close to the folded on the R.S. | 11/2 |  |  |
|  | (f) | Seam turnings trimmed to 1cm and neatened together.  | 1 |  |  |
|  | (g) | Appropriate neatening stitches use. *(If not neatened give zero from g –j)* | 1 |  |  |
|  | (h) | Evenness and correct tension of stitches. | 1 |  |  |
|  | (i) | Fastened on and off | 1 |  |  |
|  | (j) | Stitches firm and neat | 1 |  |  |
|  | (k) | Seam well presssed and flat | 1 |  |  |
|  |  | **SUB TOTAL** | **11** |  |  |
| **6.** |  | **FRONT AND BACK FACINGS** |  |  |  |
|  | (a) | Front and back facing joined with straight and firm stitchery. |  1 |  |  |
|  | (b) | Trimmed to 1cm and pressed open. | 1 |  |  |
|  | (c) | Free edge neatened with firm, smooth stitchery. | 1 |  |  |
|  | (d) | Evenness of the neatened edge. | 1 |  |  |
|  | (f) | Well pressed and flat on WS and RS | 2 |  |  |
|  |  | **SUB TOTAL** | **6** |  |  |
| **7.** |  | **PREPARATION AND ATTACHMENT OF INTERFACED COLLAR** |  |  |  |
|  | **A.** | **PREPARATION OF COLLAR** |  |  |  |
|  | (a) | Collar interfaced. | 1 |  |  |
|  | (b) | Collar joined with firm and smoothly curved stitchery. | 1 |  |  |
|  | (c) | Collar trimmed to 0.5cm all round and snipped. | 1 |  |  |
|  | (d) | Collar well knife edged. | 1 |  |  |
|  |  | **SUB TOTAL** | **4** |  |  |
|  | **B.** | **ATTACHMENT OF THE COLLAR SANDWICHING BETWEEN THE FACINGS AND GARMENT (If not give zero)** |  |  |  |
|  | (a) | Collar joined to neckline by sandwiching between the facing and garment. | 1 |  |  |
|  | (b) | Smooth and firm stitchery used. | 1 |  |  |
|  | (c) | Seam allowance trimmed and snipped. | 1 |  |  |
|  | (d) | Correct size and shape of the attached collar. | 1 |  |  |
|  | (e) | Facings, pressed appropriately. | 1 |  |  |
|  | (f) | Collar flat on both sides. | 1 |  |  |
|  |  | **SUB TOTAL** | **6** |  |  |
| **8.** |  | **BOUND OPENING** |  |  |  |
|  | (a) | Correct size of the opening. | 1 |  |  |
|  | (b) | Binding attached with firm and straight stitchery. | 1 |  |  |
|  | (c) | Raw edges neatly tucked under. | 1 |  |  |
|  | (d) | Binding held in place using appropriate stitches. | 1 |  |  |
|  | (e) | Flatness of the binding.  | 1 |  |  |
|  |  | **SUB TOTAL** | **5** |  |  |
| **9.** |  | **PREPARATION AND ATTACHMENT OF THE CUFF** |  |  |  |
|  | (a) | Cuffs joined with firm and straight stitchery. | 1 |  |  |
|  | (b) | Raw edges trimmed and corners clipped. | 1 |  |  |
|  | (c) | Well knife edged | 1 |  |  |
|  | (d) | Cuff attached to the sleeve with straight and firm stitchery. | 1 |  |  |
|  | (e) | Raw edges tucked under and held in place using appropriate stitches.  | 1 |  |  |
|  | (f) | Correct size of the complete cuff.  | 1 |  |  |
|  | (g) | Flat on W.S & R.S | 2 |  |  |
|  |  | **SUB TOTAL** | **8** |  |  |
| **10.** |  | **UNDER ARM SEAM FRENCH SEAM (I f not give zero)** |  |  |  |
|  | (a) | Straight and firm stitchery on both lines. | 2 |  |  |
|  | (b) | Raw edges completely enclosed. | 1 |  |  |
|  | (c) | Well knife edged. | 1 |  |  |
|  | (d) | Even in width. | 1 |  |  |
|  | (e) | Correct size 0.6cm to within 2mm. | 1 |  |  |
|  | (f) | Flat seam at the arm hole. | 1 |  |  |
|  | (g) | Seam pressed towards the C.B. | 1 |  |  |
|  |  | **SUB TOTAL** | **8** |  |  |
| **11.** |  | **PREPARATION AND ATTACHMENT OF THE SLEEVE** |  |  |  |
|  | (a) | Gathers made at the crown. | 1 |  |  |
|  | (b) | Gathers evenly distributed. | 1 |  |  |
|  | (c) | Sleeve attached with smoothly curved and firm stitchery. | 1 |  |  |
|  | (d) | Raw edges and notches matching. | 1 |  |  |
|  | (e) | Front sleeve joined to the front bodice and vice versa. | 1 |  |  |
|  | (f) | Seam not trimmed and not neatened. | 1 |  |  |
|  | (g) | Correct size of he seam allowance (1.5cm) | 1 |  |  |
|  | (h) | Underarm and siDe seam meeting at the armhole to within 2mm. | 1 |  |  |
|  | (j) | Good hang of the sleeve. | **1** |  |  |
|  |  | **SUB TOTAL** | **9** |  |  |
|  |  | **GRAND TOTAL** | **X/90** |  |  |