**441/2**

**HOMESCIENCE PAPER 2**

**FORM 4**

**MID TERM II 2020**

***MERU CENTRAL CLUSTER EXAMINATION***

***KENYA CERTIFICATE OF SECONDARY EDUCATION (KCSE)***

**Marking Scheme**

|  |  |  |
| --- | --- | --- |
|  | **PRESENTATION**   * Work well pressed ½ and folded ½ * Lebel (1) firmly fixed ½ on a single fabric ½ without concealing details * Pins and needles removed ½ * Tacking ½ and unnecessary hanging ½ threads removed * Made up for the left side (1) | 1  **2**  1  1  1 |
|  | **Sub Total** | **6** |
|  | **CUTTING OUT**   * All six pieces cut out ( ½ x 6) * Cutting of front bodice straight (2) and cut on grain (1) to within 2 mm * Cutting of back bodice straight (2) and cut on grain (1) * Back skirt cut straight (1) * Front skirt cut straight (1) * Smooth cutting of colar (1) and on straight grain (1) to within 2mm * Smooth cutting of the lower edge of the skirt( 2 ) front and back   ( 2 )   * Neck binding cut out on bias (1) | 3  3  3  1  1  2  4  1 |
|  | **Sub Total** | **18** |
|  | **THE DART**   * Dart made with straight stitchery (1) * Dart tapering ½ and fastened ½ at the point * Correct length of dart (1) to within 2mm(72cm – 7.6cm) * Correct width of dart (1) (mark at the seam)to within 2mm(1.2cm -1.6cm) * Flatness of dart on W.S ½ and R.S. ½ * Dart pressed towards the C.F ½ | 1  1  1  1  1  1  ( ½) |
|  | **Sub Total** | **6½** |
|  | **SEAM (OPEN SEAM)**  (if not seam give 0)   * Seam attached with straight stitchery (2) * Seam appropriately neatened (2 x 2) * Evenness of the neatened seam 2 * Correct size of seam 1 cm to within 2mm ( 0.8 – 1.2 cm) (2 x 2) * Seam open ( ½ ) and flat on R.S ( ½)and W.S (½ ) | **2**  **4**  **2**  **4**  **1½** |
|  | **Sub Total** | **13 ½** |
|  | **SIDE SEAM (BODICE AND SKIRT) FRENCH SEAM**  (If not French award 0)   * 1st line of stitching straight (1) (mark by impression) 1 x 2 * 2nd line of stitching done on the seam line (2) 1 x 2 * Evenness of the seam (2) 2 x 2 * Raw edges well concealed on the R.S (1) 1 x 2 * Correct size (width to within 2mm) (2)(0.4 – 0.8cm) 2 x 2 * Seam well knife edged (2) 2 x 2 * Flat at waist (1) 1 x 2 * Pressed towards back (at the waist) 1 x 2 | **2**  **2**  **4**  **2**  **4**  **4**  **2**  **2** |
|  | **Sub Total** | **22** |
|  | **OVERLAID SEAM**   * Straight stitchery (2) 1 x 2 close to the fold (1) 1 x 2 * Seams matching where they cross(i.e side seam of bodice and skirt) (1) * Half seam neatened (1) * Overcasting stitches done well (1) * Correct width of seam (1) (0.4 – 0.8cm) | **4**  **1**  **1**  **1**  **2** |
|  | **Sub Total** | **9** |
|  | **PREPARATION OF THE COLLOLAR AND ATTACHMENT**   * Good stitchery along the seam allowance (1) * Seam allowance trimmed to within 1mm to avoid bulk (1) * Knife edged all round (1) curves well rounded (1) * Correctly positioned 1 * Flatness of the attached collar 1 * Cross way strip even(1) and appropriately worked/hemmed (1) * Correct shape 1 and size(1) of the attached collar(super impose) * Neckline seam evenly trimmed (1) and snipped (1) * Collar attached by sandwiching between the dress ½ and cross way strip ½ | **1**  **1**  **2**  **1**  **1**  **2**  **2**  **2**  **1** |
|  | **Sub Total** | **13** |
|  | **EDGE STITCHING THE HEM**   * Straight stitchery (1) * Even edge (1) | **1**  **1** |
|  | **Sub Total** | **2** |
|  | **Grand Total** | **90** |